Autor / Author: 	Klaus Schmidt	Nr. / No.:	16-038-F
Rückfragen / Enquiries:	Klaus Schmidt	Datum / Date:	05.06.2016
Telefon / Phone:	+49 931 909-4290	E-Mail	klaus.schmidt@kba.com
Sperrvermerk / Release:		Zeichen / Ref.:	ZM/KSC
Bilder / Photographs:	2	Seiten / Pages:	1

NEO XD LR: Hybrid web press for all typical ink systems

Flexodruck with water-based inks at drupa

The new NEO XD LR HYBRID from KBA-Flexotecnica is the only CI flexo press which is demonstrating high-quality production with low-migration water-based inks at drupa. The press is engineered to print solvent-based, water-based and radiation-cured ink systems such as UV-LED or EB inks on the most varied substrates. With up to 12 printing units, printing lengths up to 1,200mm, a maximum printing width of 1,650mm and a maximum production speed of 500m/min, this CI system is state-of-the-art technology in terms of automation, makeready times, print quality and ergonomic operation. The press design also permits the retrofitting of other dryer systems to accommodate changes in market needs. Upgrades with additional flexo or gravure printing units are similarly possible. For the user, this all adds up to ultimate flexibility and a future-proof investment. KBA-Flexotecnica develops and manufactures ultra-modern CI flexo web presses for printing on paper, card, films and other flexible packaging materials. Integration into the worldwide sales and service organisation of the KBA Group guarantees close customer proximity.

Photo 1:
The CI flexo press NEO XD LR HYBRID is suitable for use with all typical ink systems

Photo 2:
Cutting-edge automation and ergonomics on the NEO XD LR